# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER (LOT 1)

**Contract title: “Supply of energy efficient equipment”**

**LOT 1: Energy efficiency measures in rooms**

**Publication reference:** BGTR0300129-SPLY-01

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1- Energy Efficiency measures: TVs (32 pcs)** | • Screen Size: 43" / 109 cm  • Image Quality: 4K Ultra HD  • Warranty Type: Official Distributor Warranty  • Resolution (Pixels): 1920 x 1080  • Display Technology: DLED  • Operating System: Android  • Quantity: 32 pieces |  |  |  |
| **2- Energy Efficiency measures: Wall type air conditioners (32 pcs)** | • Product Type: Split Air Conditioner  • Cooling Technology: Air Cooling  • Cooling Power in Watts: min: 1.00 Kw – 1.20 Kw  • Cooling Capacity(BTU/h): min: 11500 BTU/h – max: 12000 BTU/h  • Heating Capacity(BTU/h): min:13500 – max: 14000  • Internal Unit Noise Level: 35 dB(A)  • External Unit Noise Level: 48 dB(A)  • Quantity: 32 pieces |  |  |  |
| **3- Energy Efficiency measures: Hairdryers (32 pcs)** | • Power: 1600 W  • Speed Setting: 2 Stages  • Heat Setting: 2 Stages  • Warranty Type: Official Distributor Warranty  • Type: Standard  • Warranty Period: 2 Years  • Quantity: 32 pieces |  |  |  |
| **4- Energy Efficiency measures: Mini hotel type refrigerators (32 pcs)** | • Height: min: 80.00 cm – max: 90.00 cm  • Width: min: 45.00 cm – max: 50.00 cm  • Total Volume: min: 80.00 cm3 – max: 90.00 cm3  • Depth: min: 40.00 cm – max: 60.00 cm  • Energy Efficiency Class: F  • Airborne Acoustic Noise Emission: (dB (A) re 1pW) 41  • Airborne Acoustic Noise Emission: C  • Annual Energy Consumption (kWh/a): max: 150.00  • Climate Class: Extended temperate/tropical  • Quantity: 32 pieces |  |  |  |